Overview | Package | Class | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD

## com.sun.javacard.apduio
Class CadT1

    java.lang.Object
      com.sun.javacard.apduio.CadDevice
          com.sun.javacard.apduio.CadT1

Direct Known Subclasses:
  CadT1Client

    public class CadT1

extends CadDevice

The CadT1 class manages the encodes and decodes T=1 transport level messages between an InputStream and an OutputStream. This class wraps T=1 commands in a reader layer. basically, in order to send commands to the reader, a wrapper protocol has been defined. The wrapper protocol wraps message as follows: +---------+--------+---------------+-----+ | OPCODE | LENGTH | ...MESSAGE... | LRC | +---------+--------+---------------+-----+ 1 byte 2 bytes n bytes 1 byte See T1Block class for further reference.

Field Summary
`protected static int` | `MAX_IFS_SIZE`

Fields inherited from class com.sun.javacard.apduio.CadDevice
`_messages, debug, deviceProtocol, in, out, PROTOCOL_PCSC, PROTOCOL_T0, PROTOCOL_T1, PROTOCOL_TCL`

Constructor Summary
`CadT1(java.io.InputStream in, java.io.OutputStream out)` Create a new instance of the CadT1 class using an InputStream and an OutputStream.

Method Summary
`boolean` | `exchangeBlock(T1Block blockTo, T1Block blockFrom)` Implement T=1 I-block, R-block and S-block primitives Exchanges a block between the terminal and the Card reader.
`int` | `getMaxIFSSize()` Returns the maximum IFS size supported by this CAD T=1 instance.
`boolean` | `receiveBlock(T1Block blockFrom)` Reads the first T=1 Block from the terminal, setting the information inteh block passed as parameter.
`boolean` | `receivePowerUp()` Receives the power-up command from the terminal.
`byte[]` | `retrieveATR()` Receives the Aswer-To-Reset bytes from the card.
`boolean` | `sendATR(byte[] atrData)` Sends the Aswer-To-Reset bytes to the terminal.
`void` | `sendPowerDown()` Sends the power-down command to the card.
`void` | `sendPowerUp()` Sends the power-up command to the card.

Methods inherited from class com.sun.javacard.apduio.CadDevice
`close, getCadClientInstance, getDeviceProtocol, getPCSCClientInstance`

Methods inherited from class java.lang.Object
`clone, equals, finalize, getClass, hashCode, notify, notifyAll, toString, wait, wait, wait`

Field Detail

### MAX_IFS_SIZE

    protected static final int MAX_IFS_SIZE

See Also:
  Constant Field Values

Constructor Detail

### CadT1

    public CadT1(java.io.InputStream in,
                 java.io.OutputStream out)

  Create a new instance of the CadT1 class using an InputStream and an OutputStream.

  Parameters:
    `in` - The InputStream to read from.
    `out` - The OutputStream to write to.

Method Detail

### exchangeBlock

    public boolean exchangeBlock(T1Block blockTo,
                                 T1Block blockFrom)
                          throws java.io.IOException,
                                 T1Exception

  Implement T=1 I-block, R-block and S-block primitives Exchanges a block between the terminal and the Card reader.

  Parameters:
    `blockTo` - T1Block instance representing the block to send to the other entity.
    `blockFrom` - T1Block instance representing the block received from the other entity.
  Returns:
    true if the exchange compelted successfully,
    false otherwise.
  Throws:
    `T1Exception` - if a T=1 protocol or transport protocol inconsistency is detected
    `java.io.IOException` - if a problem with the I/O exchange mechanism occurs.

### receiveBlock

    public boolean receiveBlock(T1Block blockFrom)
                         throws java.io.IOException,
                                T1Exception

  Reads the first T=1 Block from the terminal, setting the information inteh block passed as parameter. Method assumes that caller is on the card side.

  Parameters:
    `blockFrom` - Block in which to receive the data.
  Throws:
    `T1Exception` - if a transport protocol inconsistency is detected.
    `java.io.IOException` - if a problem with the I/O exchange mechanism.

### sendATR

    public boolean sendATR(byte[] atrData)
                    throws java.io.IOException,
                           T1Exception

  Sends the Aswer-To-Reset bytes to the terminal. Assumes that caller is located at the Card end.

  Parameters:
    `atrData` - Byte array containing the ATR string.
  Returns:
    true if the exchange compelted successfully,
    false otherwise.
  Throws:
    `T1Exception` - if a transport protocol inconsistency is detected
    `java.io.IOException` - if a problem with the I/O exchange mechanism occurs.

### getMaxIFSSize

    public int getMaxIFSSize()

  Returns the maximum IFS size supported by this CAD T=1 instance.

  Returns:
    manimum T=1 IFS field Block size.

### retrieveATR

    public byte[] retrieveATR()
                       throws java.io.IOException,
                              T1Exception

  Receives the Aswer-To-Reset bytes from the card. Assumes that caller is located at the terminal end.

  Returns:
    byte array containing the ATR bytes from the card.
  Throws:
    `T1Exception` - if a transport protocol inconsistency is detected
    `java.io.IOException` - if a problem with the I/O exchange mechanism occurs.

### receivePowerUp

    public boolean receivePowerUp()
                           throws java.io.IOException,
                                  T1Exception

  Receives the power-up command from the terminal. Assumes that caller is located at the card end.

  Returns:
    true if the power-up command is received successfully,
    false otherwise.
  Throws:
    `T1Exception` - if a transport protocol inconsistency is detected
    `java.io.IOException` - if a problem with the I/O exchange mechanism occurs.

### sendPowerUp

    public void sendPowerUp()
                     throws java.io.IOException,
                            T1Exception

  Sends the power-up command to the card. Assumes that caller is located at the terminal end.

  Throws:
    `T1Exception` - if a transport protocol inconsistency is detected
    `java.io.IOException` - if a problem with the I/O exchange mechanism occurs.

### sendPowerDown

    public void sendPowerDown()
                       throws java.io.IOException,
                              T1Exception

  Sends the power-down command to the card. Assumes that caller is located at the terminal end.

  Throws:
    `T1Exception` - if a transport protocol inconsistency is detected
    `java.io.IOException` - if a problem with the I/O exchange mechanism occurs.

Overview | Package | Class | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD

Copyright (c) 2009 Sun Microsystems, Inc. All rights reserved.