Overview | Package | Class | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD

## com.sun.javacard.apduio
Class CadT1Dual

    java.lang.Object
      com.sun.javacard.apduio.CadT1Dual

    public class CadT1Dual

extends java.lang.Object

The CadT1Dual class manages two T1 connections It uses two instances of ServerT1Data to store status of the protocols Two initialize the class, use constructor with contacted socket and set contacted_atr It contactless connection is also available, set also contactless socket and contactless atr This class uses two instances of T1BlockReade to listen to incoming blocks

Field Summary
`protected static int` | `MAX_IFS_SIZE`

Constructor Summary
`CadT1Dual(java.net.Socket contactedSocket)` Create a new instance of the CadT1 class using socket representing the contacted connection.

Method Summary
`void` | `addCadServerListener(CadServerListener listener)` Register a new CadServerListener to be notified of state changes.
`static void` | `discardIncomingGetLe(CadT1Dual cadObj, short[] LEN, short numBytesExpected, short numBytesReceived)`
`byte` | `getActiveInterface()`
`int` | `getMaxIFSSize()` Returns the maximum IFS size supported by this CAD T=1 instance.
`byte` | `getSecondaryInterfaceEvent()`
`static void` | `placeDataInBuffer(CadT1Dual cadObj, byte[] bufferINF, short[] LEN, short offset, short buffSize)`
`boolean` | `receiveBlock(T1Block blockFrom, boolean switchInterface)` Reads the first T=1 Block from the terminal, setting the information inteh block passed as parameter.
`void` | `setContactedATR(byte[] contacted_atr)`
`void` | `setContactlessATR(byte[] contactless_atr)`
`void` | `setContactlessSocket(java.net.Socket contactlessSocket)`
`boolean` | `t1Abort()`
`short` | `t1GetIFSC()` This method returns the T=1 maximum supported card Information Field block size (IFSC).
`short` | `t1GetIFSD()` This method returns the T=1 maximum supported device Information Field block size (IFSD).
`static byte` | `t1GetNAD()` This method returns the T=1 NAD byte for the last block received.
`boolean` | `t1LastBlockReceived()` This method returns true if the last T=1 block in a chain has been received (i.e.
`short` | `t1RcvBlock(byte[] bufferINF, short[] LEN, short offset, short buffSize)` This method receives a T=1 block of data - if none are pending - or copies the data of an already- received block into the APDU buffer at the offset specified.
`short` | `t1SndBlockRcvAck(byte[] buffer, int dataOffset, int dataLength, boolean isLastBlock, boolean switchInterface)` This method sends a T=1 block data in the APDU buffer specified bythe offset and length passed, and waits for acknowledgement transmission, without copying any data that might come along on that transmission.
`boolean` | `t1Wait()` This method initiates a T=1 wait sequence to indicate the terminal that more time is required to process input, and thus avoid a timeout.

Methods inherited from class java.lang.Object
`clone, equals, finalize, getClass, hashCode, notify, notifyAll, toString, wait, wait, wait`

Field Detail

### MAX_IFS_SIZE

    protected static final int MAX_IFS_SIZE

See Also:
  Constant Field Values

Constructor Detail

### CadT1Dual

    public CadT1Dual(java.net.Socket contactedSocket)

  Create a new instance of the CadT1 class using socket representing the contacted connection.

  Parameters:
    `contactedSocket` -

Method Detail

### setContactedATR

    public void setContactedATR(byte[] contacted_atr)

  Parameters:
    `contacted_atr` -

### setContactlessATR

    public void setContactlessATR(byte[] contactless_atr)

  Parameters:
    `contactless_atr` -

### getSecondaryInterfaceEvent

    public byte getSecondaryInterfaceEvent()

  Returns:

### getActiveInterface

    public byte getActiveInterface()

  Returns:

### setContactlessSocket

    public void setContactlessSocket(java.net.Socket contactlessSocket)

  Parameters:
    `contactlessSocket` -

### receiveBlock

    public boolean receiveBlock(T1Block blockFrom,
                                boolean switchInterface)
                         throws java.io.IOException,
                                T1Exception

  Reads the first T=1 Block from the terminal, setting the information inteh block passed as parameter. Method assumes that caller is on the card side.

  Parameters:
    `switchInterface` -
    `blockFrom` - Block in which to receive the data.
  Returns:
  Throws:
    `T1Exception` - if a transport protocol inconsistency is detected.
    `java.io.IOException` - if a problem with the I/O exchange mechanism.

### getMaxIFSSize

    public int getMaxIFSSize()

  Returns the maximum IFS size supported by this CAD T=1 instance.

  Returns:
    manimum T=1 IFS field Block size.

### t1Wait

    public boolean t1Wait()
                   throws T1Exception

  This method initiates a T=1 wait sequence to indicate the terminal that more time is required to process input, and thus avoid a timeout. Only Java Card runtime environment can invoke this method.

  Returns:
    0 on success.
  Throws:
    `T1Exception`

### t1Abort

    public boolean t1Abort()
                    throws T1Exception

  Throws:
    `T1Exception`

### t1LastBlockReceived

    public boolean t1LastBlockReceived()

  This method returns
  true if the last T=1 block in a chain has been received (i.e. block with the M bit set to 1),
  false otherwise. Only Java Card runtime environment can invoke this method.

  Returns:
    true if last block recevied,
    false otherwise.

### addCadServerListener

    public void addCadServerListener(CadServerListener listener)

  Register a new CadServerListener to be notified of state changes.

  Parameters:
    `listener` - The listener to register.

### discardIncomingGetLe

    public static void discardIncomingGetLe(CadT1Dual cadObj,
                                            short[] LEN,
                                            short numBytesExpected,
                                            short numBytesReceived)

### placeDataInBuffer

    public static void placeDataInBuffer(CadT1Dual cadObj,
                                         byte[] bufferINF,
                                         short[] LEN,
                                         short offset,
                                         short buffSize)

### t1SndBlockRcvAck

    public short t1SndBlockRcvAck(byte[] buffer,
                                  int dataOffset,
                                  int dataLength,
                                  boolean isLastBlock,
                                  boolean switchInterface)
                           throws T1Exception

  This method sends a T=1 block data in the APDU buffer specified bythe offset and length passed, and waits for acknowledgement transmission, without copying any data that might come along on that transmission. On dual interface cards, the acknowledgement might come from a different interface if the interface is not locked. Only Java Card runtime environment can invoke this method.

  Parameters:
    `buffer` - Data buffer
    `dataOffset` - offset to data
    `dataLength` - length of data
    `isLastBlock` - last block of APDU flag
    `switchInterface` - OK to switch interface
  Returns:
    0 on success, other value in error.
  Throws:
    `T1Exception`

### t1RcvBlock

    public short t1RcvBlock(byte[] bufferINF,
                            short[] LEN,
                            short offset,
                            short buffSize)
                     throws T1Exception

  This method receives a T=1 block of data - if none are pending - or copies the data of an already- received block into the APDU buffer at the offset specified. If the data cannot fit into the APDU buffer, the remaining data will be copied the next time this method is called. Only Java Card runtime environment can invoke this method.

  Parameters:
    `bufferINF` -
    `LEN` -
    `offset` -
    `buffSize` -
  Returns:
    number of bytes received on success, negative values on error.
  Throws:
    `T1Exception`

### t1GetNAD

    public static byte t1GetNAD()

  This method returns the T=1 NAD byte for the last block received. Only Java Card runtime environment can invoke this method.

  Returns:
    T=1 NAD value.

### t1GetIFSC

    public short t1GetIFSC()

  This method returns the T=1 maximum supported card Information Field block size (IFSC). Only Java Card runtime environment can invoke this method.

  Returns:
    T=1 IFSC value.

### t1GetIFSD

    public short t1GetIFSD()

  This method returns the T=1 maximum supported device Information Field block size (IFSD). Only Java Card runtime environment can invoke this method.

  Returns:
    T=1 IFSD value.

Overview | Package | Class | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD

Copyright (c) 2009 Sun Microsystems, Inc. All rights reserved.