Public Attributes

# IMediumAttachment Interface Reference

The IMediumAttachment interface links storage media to virtual machines. More...

List of all members.

## Public Attributes
readonly attribute IMedium | medium
| Medium object associated with this attachment; it can be `null` for removable devices.
readonly attribute wstring | controller
| Name of the storage controller of this attachment; this refers to one of the controllers in IMachine::storageControllers by name.
readonly attribute long | port
| Port number of this attachment.
readonly attribute long | device
| Device slot number of this attachment.
readonly attribute DeviceType | type
| Device type of this attachment.
readonly attribute boolean | passthrough
| Pass I/O requests through to a device on the host.
readonly attribute boolean | temporaryEject
| Whether guest-triggered eject results in unmounting the medium.
readonly attribute boolean | isEjected
| Signals that the removable medium has been ejected.
readonly attribute boolean | nonRotational
| Whether the associated medium is non-rotational.
readonly attribute IBandwidthGroup | bandwidthGroup
| The bandwidth group this medium attachment is assigned to.

## Detailed Description

The IMediumAttachment interface links storage media to virtual machines.

For each medium (IMedium) which has been attached to a storage controller (IStorageController) of a machine (IMachine) via the IMachine::attachDevice method, one instance of IMediumAttachment is added to the machine's IMachine::mediumAttachments array attribute.

Each medium attachment specifies the storage controller as well as a port and device number and the IMedium instance representing a virtual hard disk or floppy or DVD image.

For removable media (DVDs or floppies), there are two additional options. For one, the IMedium instance can be `null` to represent an empty drive with no media inserted (see IMachine::mountMedium); secondly, the medium can be one of the pseudo-media for host drives listed in IHost::DVDDrives or IHost::floppyDrives.

### Attaching Hard Disks

Hard disks are attached to virtual machines using the IMachine::attachDevice method and detached using the IMachine::detachDevice method. Depending on a medium's type (see IMedium::type), hard disks are attached either directly or indirectly.

When a hard disk is being attached directly, it is associated with the virtual machine and used for hard disk operations when the machine is running. When a hard disk is being attached indirectly, a new differencing hard disk linked to it is implicitly created and this differencing hard disk is associated with the machine and used for hard disk operations. This also means that if IMachine::attachDevice performs a direct attachment then the same hard disk will be returned in response to the subsequent IMachine::getMedium call; however if an indirect attachment is performed then IMachine::getMedium will return the implicitly created differencing hard disk, not the original one passed to IMachine::attachDevice. In detail:

- Normal base hard disks that do not have children (i.e. differencing hard disks linked to them) and that are not already attached to virtual machines in snapshots are attached directly. Otherwise, they are attached indirectly because having dependent children or being part of the snapshot makes it impossible to modify hard disk contents without breaking the integrity of the dependent party. The IMedium::readOnly attribute allows to quickly determine the kind of the attachment for the given hard disk. Note that if a normal base hard disk is to be indirectly attached to a virtual machine with snapshots then a special procedure called smart attachment is performed (see below).
- Normal differencing hard disks are like normal base hard disks: they are attached directly if they do not have children and are not attached to virtual machines in snapshots, and indirectly otherwise. Note that the smart attachment procedure is never performed for differencing hard disks.
- Immutable hard disks are always attached indirectly because they are designed to be non-writable. If an immutable hard disk is attached to a virtual machine with snapshots then a special procedure called smart attachment is performed (see below).
- Writethrough hard disks are always attached directly, also as designed. This also means that writethrough hard disks cannot have other hard disks linked to them at all.
- Shareable hard disks are always attached directly, also as designed. This also means that shareable hard disks cannot have other hard disks linked to them at all. They behave almost like writethrough hard disks, except that shareable hard disks can be attached to several virtual machines which are running, allowing concurrent accesses. You need special cluster software running in the virtual machines to make use of such disks.

Note that the same hard disk, regardless of its type, may be attached to more than one virtual machine at a time. In this case, the machine that is started first gains exclusive access to the hard disk and attempts to start other machines having this hard disk attached will fail until the first machine is powered down.

Detaching hard disks is performed in a deferred fashion. This means that the given hard disk remains associated with the given machine after a successful IMachine::detachDevice call until IMachine::saveSettings is called to save all changes to machine settings to disk. This deferring is necessary to guarantee that the hard disk configuration may be restored at any time by a call to IMachine::discardSettings before the settings are saved (committed).

Note that if IMachine::discardSettings is called after indirectly attaching some hard disks to the machine but before a call to IMachine::saveSettings is made, it will implicitly delete all differencing hard disks implicitly created by IMachine::attachDevice for these indirect attachments. Such implicitly created hard disks will also be immediately deleted when detached explicitly using the IMachine::detachDevice call if it is made before IMachine::saveSettings. This implicit deletion is safe because newly created differencing hard disks do not contain any user data.

However, keep in mind that detaching differencing hard disks that were implicitly created by IMachine::attachDevice before the last IMachine::saveSettings call will not implicitly delete them as they may already contain some data (for example, as a result of virtual machine execution). If these hard disks are no more necessary, the caller can always delete them explicitly using IMedium::deleteStorage after they are actually de-associated from this machine by the IMachine::saveSettings call.

### Smart Attachment

When normal base or immutable hard disks are indirectly attached to a virtual machine then some additional steps are performed to make sure the virtual machine will have the most recent "view" of the hard disk being attached. These steps include walking through the machine's snapshots starting from the current one and going through ancestors up to the first snapshot. Hard disks attached to the virtual machine in all of the encountered snapshots are checked whether they are descendants of the given normal base or immutable hard disk. The first found child (which is the differencing hard disk) will be used instead of the normal base or immutable hard disk as a parent for creating a new differencing hard disk that will be actually attached to the machine. And only if no descendants are found or if the virtual machine does not have any snapshots then the normal base or immutable hard disk will be used itself as a parent for this differencing hard disk.

It is easier to explain what smart attachment does using the following example:

    BEFORE attaching B.vdi:       AFTER attaching B.vdi:

    Snapshot 1 (B.vdi)            Snapshot 1 (B.vdi)
     Snapshot 2 (D1->B.vdi)        Snapshot 2 (D1->B.vdi)
      Snapshot 3 (D2->D1.vdi)       Snapshot 3 (D2->D1.vdi)
       Snapshot 4 (none)             Snapshot 4 (none)
        CurState   (none)             CurState   (D3->D2.vdi)

                                  NOT
                                     ...
                                      CurState   (D3->B.vdi)

The first column is the virtual machine configuration before the base hard disk `B.vdi` is attached, the second column shows the machine after this hard disk is attached. Constructs like `D1->B.vdi` and similar mean that the hard disk that is actually attached to the machine is a differencing hard disk, `D1.vdi`, which is linked to (based on) another hard disk, `B.vdi`.

As we can see from the example, the hard disk `B.vdi` was detached from the machine before taking Snapshot 4. Later, after Snapshot 4 was taken, the user decides to attach `B.vdi` again. `B.vdi` has dependent child hard disks (`D1.vdi`, `D2.vdi`), therefore it cannot be attached directly and needs an indirect attachment (i.e. implicit creation of a new differencing hard disk). Due to the smart attachment procedure, the new differencing hard disk (`D3.vdi`) will be based on `D2.vdi`, not on `B.vdi` itself, since `D2.vdi` is the most recent view of `B.vdi` existing for this snapshot branch of the given virtual machine.

Note that if there is more than one descendant hard disk of the given base hard disk found in a snapshot, and there is an exact device, channel and bus match, then this exact match will be used. Otherwise, the youngest descendant will be picked up.

There is one more important aspect of the smart attachment procedure which is not related to snapshots at all. Before walking through the snapshots as described above, the backup copy of the current list of hard disk attachment is searched for descendants. This backup copy is created when the hard disk configuration is changed for the first time after the last IMachine::saveSettings call and used by IMachine::discardSettings to undo the recent hard disk changes. When such a descendant is found in this backup copy, it will be simply re-attached back, without creating a new differencing hard disk for it. This optimization is necessary to make it possible to re-attach the base or immutable hard disk to a different bus, channel or device slot without losing the contents of the differencing hard disk actually attached to the machine in place of it.

Interface ID:
  `{B5DFBB8C-7498-48C3-BF10-78FC60F064E1}`

## Member Data Documentation

readonly attribute IMedium IMediumAttachment::medium

Medium object associated with this attachment; it can be `null` for removable devices.

readonly attribute wstring IMediumAttachment::controller

Name of the storage controller of this attachment; this refers to one of the controllers in IMachine::storageControllers by name.

readonly attribute long IMediumAttachment::port

Port number of this attachment.

See IMachine::attachDevice for the meaning of this value for the different controller types.

readonly attribute long IMediumAttachment::device

Device slot number of this attachment.

See IMachine::attachDevice for the meaning of this value for the different controller types.

readonly attribute DeviceType IMediumAttachment::type

Device type of this attachment.

readonly attribute boolean IMediumAttachment::passthrough

Pass I/O requests through to a device on the host.

readonly attribute boolean IMediumAttachment::temporaryEject

Whether guest-triggered eject results in unmounting the medium.

readonly attribute boolean IMediumAttachment::isEjected

Signals that the removable medium has been ejected.

This is not necessarily equivalent to having a `null` medium association.

readonly attribute boolean IMediumAttachment::nonRotational

Whether the associated medium is non-rotational.

readonly attribute IBandwidthGroup IMediumAttachment::bandwidthGroup

The bandwidth group this medium attachment is assigned to.