# utf8.h File Reference

C API: 8-bit Unicode handling macros. More...

`#include "unicode/utf.h"`

Go to the source code of this file.

## Defines
#define | U8_COUNT_TRAIL_BYTES(leadByte) (utf8_countTrailBytes[(uint8_t)leadByte])
| Count the trail bytes for a UTF-8 lead byte.
#define | U8_MASK_LEAD_BYTE(leadByte, countTrailBytes) ((leadByte)&=(1<<(6-(countTrailBytes)))-1)
| Mask a UTF-8 lead byte, leave only the lower bits that form part of the code point value.
#define | U8_IS_SINGLE(c) (((c)&0x80)==0)
| Does this code unit (byte) encode a code point by itself (US-ASCII 0.
#define | U8_IS_LEAD(c) ((uint8_t)((c)-0xc0)<0x3e)
| Is this code unit (byte) a UTF-8 lead byte?
#define | U8_IS_TRAIL(c) (((c)&0xc0)==0x80)
| Is this code unit (byte) a UTF-8 trail byte?
#define | U8_LENGTH(c)
| How many code units (bytes) are used for the UTF-8 encoding of this Unicode code point?
#define | U8_MAX_LENGTH 4
| The maximum number of UTF-8 code units (bytes) per Unicode code point (U+0000.
#define | U8_GET_UNSAFE(s, i, c)
| Get a code point from a string at a random-access offset, without changing the offset.
#define | U8_GET(s, start, i, length, c)
| Get a code point from a string at a random-access offset, without changing the offset.
#define | U8_NEXT_UNSAFE(s, i, c)
| Get a code point from a string at a code point boundary offset, and advance the offset to the next code point boundary.
#define | U8_NEXT(s, i, length, c)
| Get a code point from a string at a code point boundary offset, and advance the offset to the next code point boundary.
#define | U8_APPEND_UNSAFE(s, i, c)
| Append a code point to a string, overwriting 1 to 4 bytes.
#define | U8_APPEND(s, i, capacity, c, isError)
| Append a code point to a string, overwriting 1 to 4 bytes.
#define | U8_FWD_1_UNSAFE(s, i)
| Advance the string offset from one code point boundary to the next.
#define | U8_FWD_1(s, i, length)
| Advance the string offset from one code point boundary to the next.
#define | U8_FWD_N_UNSAFE(s, i, n)
| Advance the string offset from one code point boundary to the n-th next one, i.e., move forward by n code points.
#define | U8_FWD_N(s, i, length, n)
| Advance the string offset from one code point boundary to the n-th next one, i.e., move forward by n code points.
#define | U8_SET_CP_START_UNSAFE(s, i)
| Adjust a random-access offset to a code point boundary at the start of a code point.
#define | U8_SET_CP_START(s, start, i)
| Adjust a random-access offset to a code point boundary at the start of a code point.
#define | U8_PREV_UNSAFE(s, i, c)
| Move the string offset from one code point boundary to the previous one and get the code point between them.
#define | U8_PREV(s, start, i, c)
| Move the string offset from one code point boundary to the previous one and get the code point between them.
#define | U8_BACK_1_UNSAFE(s, i)
| Move the string offset from one code point boundary to the previous one.
#define | U8_BACK_1(s, start, i)
| Move the string offset from one code point boundary to the previous one.
#define | U8_BACK_N_UNSAFE(s, i, n)
| Move the string offset from one code point boundary to the n-th one before it, i.e., move backward by n code points.
#define | U8_BACK_N(s, start, i, n)
| Move the string offset from one code point boundary to the n-th one before it, i.e., move backward by n code points.
#define | U8_SET_CP_LIMIT_UNSAFE(s, i)
| Adjust a random-access offset to a code point boundary after a code point.
#define | U8_SET_CP_LIMIT(s, start, i, length)
| Adjust a random-access offset to a code point boundary after a code point.
## Functions
UChar32 | utf8_nextCharSafeBody (const uint8_t *s, int32_t *pi, int32_t length, UChar32 c, UBool strict)
| Function for handling "next code point" with error-checking.
int32_t | utf8_appendCharSafeBody (uint8_t *s, int32_t i, int32_t length, UChar32 c, UBool *pIsError)
| Function for handling "append code point" with error-checking.
UChar32 | utf8_prevCharSafeBody (const uint8_t *s, int32_t start, int32_t *pi, UChar32 c, UBool strict)
| Function for handling "previous code point" with error-checking.
int32_t | utf8_back1SafeBody (const uint8_t *s, int32_t start, int32_t i)
| Function for handling "skip backward one code point" with error-checking.
## Variables
U_CFUNC U_IMPORT const uint8_t | utf8_countTrailBytes [256]
| Internal array with numbers of trail bytes for any given byte used in lead byte position.

## Detailed Description

C API: 8-bit Unicode handling macros.

This file defines macros to deal with 8-bit Unicode (UTF-8) code units (bytes) and strings. utf8.h is included by utf.h after unicode/umachine.h and some common definitions.

For more information see utf.h and the ICU User Guide Strings chapter (http://icu-project.org/userguide/strings.html).

Usage: ICU coding guidelines for if() statements should be followed when using these macros. Compound statements (curly braces {}) must be used for if-else-while... bodies and all macro statements should be terminated with semicolon.

Definition in file utf8.h.

## Define Documentation

#define U8_APPEND | ( | s,
|  | i,
|  | capacity,
|  | c,
|  | isError |  | ) |

Value:

    { \
        if((uint32_t)(c)<=0x7f) { \
            (s)[(i)++]=(uint8_t)(c); \
        } else if((uint32_t)(c)<=0x7ff && (i)+1<(capacity)) { \
            (s)[(i)++]=(uint8_t)(((c)>>6)|0xc0); \
            (s)[(i)++]=(uint8_t)(((c)&0x3f)|0x80); \
        } else if((uint32_t)(c)<=0xd7ff && (i)+2<(capacity)) { \
            (s)[(i)++]=(uint8_t)(((c)>>12)|0xe0); \
            (s)[(i)++]=(uint8_t)((((c)>>6)&0x3f)|0x80); \
            (s)[(i)++]=(uint8_t)(((c)&0x3f)|0x80); \
        } else { \
            (i)=utf8_appendCharSafeBody(s, (int32_t)(i), (int32_t)(capacity), c, &(isError)); \
        } \
    }

Append a code point to a string, overwriting 1 to 4 bytes.

The offset points to the current end of the string contents and is advanced (post-increment). "Safe" macro, checks for a valid code point. If a non-ASCII code point is written, checks for sufficient space in the string. If the code point is not valid or trail bytes do not fit, then isError is set to TRUE.

Parameters:

  | s | const uint8_t * string buffer
  | i | string offset, must be i<capacity
  | capacity | size of the string buffer
  | c | code point to append
  | isError | output UBool set to TRUE if an error occurs, otherwise not modified

See also:
  U8_APPEND_UNSAFE

Stable:
  ICU 2.4

Definition at line 330 of file utf8.h.

#define U8_APPEND_UNSAFE | ( | s,
|  | i,
|  | c |  | ) |

Value:

    { \
        if((uint32_t)(c)<=0x7f) { \
            (s)[(i)++]=(uint8_t)(c); \
        } else { \
            if((uint32_t)(c)<=0x7ff) { \
                (s)[(i)++]=(uint8_t)(((c)>>6)|0xc0); \
            } else { \
                if((uint32_t)(c)<=0xffff) { \
                    (s)[(i)++]=(uint8_t)(((c)>>12)|0xe0); \
                } else { \
                    (s)[(i)++]=(uint8_t)(((c)>>18)|0xf0); \
                    (s)[(i)++]=(uint8_t)((((c)>>12)&0x3f)|0x80); \
                } \
                (s)[(i)++]=(uint8_t)((((c)>>6)&0x3f)|0x80); \
            } \
            (s)[(i)++]=(uint8_t)(((c)&0x3f)|0x80); \
        } \
    }

Append a code point to a string, overwriting 1 to 4 bytes.

The offset points to the current end of the string contents and is advanced (post-increment). "Unsafe" macro, assumes a valid code point and sufficient space in the string. Otherwise, the result is undefined.

Parameters:

  | s | const uint8_t * string buffer
  | i | string offset
  | c | code point to append

See also:
  U8_APPEND

Stable:
  ICU 2.4

Definition at line 294 of file utf8.h.

#define U8_BACK_1 | ( | s,
|  | start,
|  | i |  | ) |

Value:

    { \
        if(U8_IS_TRAIL((s)[--(i)])) { \
            (i)=utf8_back1SafeBody(s, start, (int32_t)(i)); \
        } \
    }

Move the string offset from one code point boundary to the previous one.

(Pre-decrementing backward iteration.) The input offset may be the same as the string length. "Safe" macro, checks for illegal sequences and for string boundaries.

Parameters:

  | s | const uint8_t * string
  | start | starting string offset (usually 0)
  | i | string offset, must be start<i

See also:
  U8_BACK_1_UNSAFE

Stable:
  ICU 2.4

Definition at line 563 of file utf8.h.

#define U8_BACK_1_UNSAFE | ( | s,
|  | i |  | ) |

Value:

    { \
        while(U8_IS_TRAIL((s)[--(i)])) {} \
    }

Move the string offset from one code point boundary to the previous one.

(Pre-decrementing backward iteration.) The input offset may be the same as the string length. "Unsafe" macro, assumes well-formed UTF-8.

Parameters:

  | s | const uint8_t * string
  | i | string offset

See also:
  U8_BACK_1

Stable:
  ICU 2.4

Definition at line 547 of file utf8.h.

#define U8_BACK_N | ( | s,
|  | start,
|  | i,
|  | n |  | ) |

Value:

    { \
        int32_t __N=(n); \
        while(__N>0 && (i)>(start)) { \
            U8_BACK_1(s, start, i); \
            --__N; \
        } \
    }

Move the string offset from one code point boundary to the n-th one before it, i.e., move backward by n code points.

(Pre-decrementing backward iteration.) The input offset may be the same as the string length. "Safe" macro, checks for illegal sequences and for string boundaries.

Parameters:

  | s | const uint8_t * string
  | start | index of the start of the string
  | i | string offset, must be start<i
  | n | number of code points to skip

See also:
  U8_BACK_N_UNSAFE

Stable:
  ICU 2.4

Definition at line 604 of file utf8.h.

#define U8_BACK_N_UNSAFE | ( | s,
|  | i,
|  | n |  | ) |

Value:

    { \
        int32_t __N=(n); \
        while(__N>0) { \
            U8_BACK_1_UNSAFE(s, i); \
            --__N; \
        } \
    }

Move the string offset from one code point boundary to the n-th one before it, i.e., move backward by n code points.

(Pre-decrementing backward iteration.) The input offset may be the same as the string length. "Unsafe" macro, assumes well-formed UTF-8.

Parameters:

  | s | const uint8_t * string
  | i | string offset
  | n | number of code points to skip

See also:
  U8_BACK_N

Stable:
  ICU 2.4

Definition at line 582 of file utf8.h.

#define U8_COUNT_TRAIL_BYTES | ( | leadByte |  | ) | (utf8_countTrailBytes[(uint8_t)leadByte])

Count the trail bytes for a UTF-8 lead byte.

Internal:
  Do not use. This API is for internal use only.

Definition at line 63 of file utf8.h.

#define U8_FWD_1 | ( | s,
|  | i,
|  | length |  | ) |

Value:

    { \
        uint8_t __b=(uint8_t)(s)[(i)++]; \
        if(U8_IS_LEAD(__b)) { \
            uint8_t __count=U8_COUNT_TRAIL_BYTES(__b); \
            if((i)+__count>(length)) { \
                __count=(uint8_t)((length)-(i)); \
            } \
            while(__count>0 && U8_IS_TRAIL((s)[i])) { \
                ++(i); \
                --__count; \
            } \
        } \
    }

Advance the string offset from one code point boundary to the next.

(Post-incrementing iteration.) "Safe" macro, checks for illegal sequences and for string boundaries.

Parameters:

  | s | const uint8_t * string
  | i | string offset, must be i<length
  | length | string length

See also:
  U8_FWD_1_UNSAFE

Stable:
  ICU 2.4

Definition at line 370 of file utf8.h.

#define U8_FWD_1_UNSAFE | ( | s,
|  | i |  | ) |

Value:

    { \
        (i)+=1+U8_COUNT_TRAIL_BYTES((s)[i]); \
    }

Advance the string offset from one code point boundary to the next.

(Post-incrementing iteration.) "Unsafe" macro, assumes well-formed UTF-8.

Parameters:

  | s | const uint8_t * string
  | i | string offset

See also:
  U8_FWD_1

Stable:
  ICU 2.4

Definition at line 355 of file utf8.h.

#define U8_FWD_N | ( | s,
|  | i,
|  | length,
|  | n |  | ) |

Value:

    { \
        int32_t __N=(n); \
        while(__N>0 && (i)<(length)) { \
            U8_FWD_1(s, i, length); \
            --__N; \
        } \
    }

Advance the string offset from one code point boundary to the n-th next one, i.e., move forward by n code points.

(Post-incrementing iteration.) "Safe" macro, checks for illegal sequences and for string boundaries.

Parameters:

  | s | const uint8_t * string
  | i | string offset, must be i<length
  | length | string length
  | n | number of code points to skip

See also:
  U8_FWD_N_UNSAFE

Stable:
  ICU 2.4

Definition at line 417 of file utf8.h.

#define U8_FWD_N_UNSAFE | ( | s,
|  | i,
|  | n |  | ) |

Value:

    { \
        int32_t __N=(n); \
        while(__N>0) { \
            U8_FWD_1_UNSAFE(s, i); \
            --__N; \
        } \
    }

Advance the string offset from one code point boundary to the n-th next one, i.e., move forward by n code points.

(Post-incrementing iteration.) "Unsafe" macro, assumes well-formed UTF-8.

Parameters:

  | s | const uint8_t * string
  | i | string offset
  | n | number of code points to skip

See also:
  U8_FWD_N

Stable:
  ICU 2.4

Definition at line 396 of file utf8.h.

#define U8_GET | ( | s,
|  | start,
|  | i,
|  | length,
|  | c |  | ) |

Value:

    { \
        int32_t _u8_get_index=(int32_t)(i); \
        U8_SET_CP_START(s, start, _u8_get_index); \
        U8_NEXT(s, _u8_get_index, length, c); \
    }

Get a code point from a string at a random-access offset, without changing the offset.

The offset may point to either the lead byte or one of the trail bytes for a code point, in which case the macro will read all of the bytes for the code point. If the offset points to an illegal UTF-8 byte sequence, then c is set to a negative value. Iteration through a string is more efficient with U8_NEXT_UNSAFE or U8_NEXT.

Parameters:

  | s | const uint8_t * string
  | start | starting string offset
  | i | string offset, must be start<=i<length
  | length | string length
  | c | output UChar32 variable, set to <0 in case of an error

See also:
  U8_GET_UNSAFE

Stable:
  ICU 2.4

Definition at line 190 of file utf8.h.

#define U8_GET_UNSAFE | ( | s,
|  | i,
|  | c |  | ) |

Value:

    { \
        int32_t _u8_get_unsafe_index=(int32_t)(i); \
        U8_SET_CP_START_UNSAFE(s, _u8_get_unsafe_index); \
        U8_NEXT_UNSAFE(s, _u8_get_unsafe_index, c); \
    }

Get a code point from a string at a random-access offset, without changing the offset.

The offset may point to either the lead byte or one of the trail bytes for a code point, in which case the macro will read all of the bytes for the code point. The result is undefined if the offset points to an illegal UTF-8 byte sequence. Iteration through a string is more efficient with U8_NEXT_UNSAFE or U8_NEXT.

Parameters:

  | s | const uint8_t * string
  | i | string offset
  | c | output UChar32 variable

See also:
  U8_GET

Stable:
  ICU 2.4

Definition at line 166 of file utf8.h.

#define U8_IS_LEAD | ( | c |  | ) | ((uint8_t)((c)-0xc0)<0x3e)

Is this code unit (byte) a UTF-8 lead byte?

Parameters:

  | c | 8-bit code unit (byte)

Returns:
  TRUE or FALSE

Stable:
  ICU 2.4

Definition at line 115 of file utf8.h.

#define U8_IS_SINGLE | ( | c |  | ) | (((c)&0x80)==0)

Does this code unit (byte) encode a code point by itself (US-ASCII 0.

.0x7f)?

Parameters:

  | c | 8-bit code unit (byte)

Returns:
  TRUE or FALSE

Stable:
  ICU 2.4

Definition at line 107 of file utf8.h.

#define U8_IS_TRAIL | ( | c |  | ) | (((c)&0xc0)==0x80)

Is this code unit (byte) a UTF-8 trail byte?

Parameters:

  | c | 8-bit code unit (byte)

Returns:
  TRUE or FALSE

Stable:
  ICU 2.4

Definition at line 123 of file utf8.h.

#define U8_LENGTH | ( | c |  | ) |

Value:

    ((uint32_t)(c)<=0x7f ? 1 : \
            ((uint32_t)(c)<=0x7ff ? 2 : \
                ((uint32_t)(c)<=0xd7ff ? 3 : \
                    ((uint32_t)(c)<=0xdfff || (uint32_t)(c)>0x10ffff ? 0 : \
                        ((uint32_t)(c)<=0xffff ? 3 : 4)\
                    ) \
                ) \
            ) \
        )

How many code units (bytes) are used for the UTF-8 encoding of this Unicode code point?

Parameters:

  | c | 32-bit code point

Returns:
  1..4, or 0 if c is a surrogate or not a Unicode code point

Stable:
  ICU 2.4

Definition at line 132 of file utf8.h.

#define U8_MASK_LEAD_BYTE | ( | leadByte,
|  | countTrailBytes |  | ) | ((leadByte)&=(1<<(6-(countTrailBytes)))-1)

Mask a UTF-8 lead byte, leave only the lower bits that form part of the code point value.

Internal:
  Do not use. This API is for internal use only.

Definition at line 69 of file utf8.h.

#define U8_MAX_LENGTH 4

The maximum number of UTF-8 code units (bytes) per Unicode code point (U+0000.

.U+10ffff).

Returns:
  4

Stable:
  ICU 2.4

Definition at line 148 of file utf8.h.

#define U8_NEXT | ( | s,
|  | i,
|  | length,
|  | c |  | ) |

Value:

    { \
        (c)=(uint8_t)(s)[(i)++]; \
        if((c)>=0x80) { \
            uint8_t __t1, __t2; \
            if( /* handle U+1000..U+CFFF inline */ \
                (0xe0<(c) && (c)<=0xec) && \
                (((i)+1)<(length)) && \
                (__t1=(uint8_t)((s)[i]-0x80))<=0x3f && \
                (__t2=(uint8_t)((s)[(i)+1]-0x80))<= 0x3f \
            ) { \
                /* no need for (c&0xf) because the upper bits are truncated after <<12 in the cast to (UChar) */ \
                (c)=(UChar)(((c)<<12)|(__t1<<6)|__t2); \
                (i)+=2; \
            } else if( /* handle U+0080..U+07FF inline */ \
                ((c)<0xe0 && (c)>=0xc2) && \
                ((i)<(length)) && \
                (__t1=(uint8_t)((s)[i]-0x80))<=0x3f \
            ) { \
                (c)=(UChar)((((c)&0x1f)<<6)|__t1); \
                ++(i); \
            } else if(U8_IS_LEAD(c)) { \
                /* function call for "complicated" and error cases */ \
                (c)=utf8_nextCharSafeBody((const uint8_t *)s, &(i), (int32_t)(length), c, -1); \
            } else { \
                (c)=U_SENTINEL; \
            } \
        } \
    }

Get a code point from a string at a code point boundary offset, and advance the offset to the next code point boundary.

(Post-incrementing forward iteration.) "Safe" macro, checks for illegal sequences and for string boundaries.

The offset may point to the lead byte of a multi-byte sequence, in which case the macro will read the whole sequence. If the offset points to a trail byte or an illegal UTF-8 sequence, then c is set to a negative value.

Parameters:

  | s | const uint8_t * string
  | i | string offset, must be i<length
  | length | string length
  | c | output UChar32 variable, set to <0 in case of an error

See also:
  U8_NEXT_UNSAFE

Stable:
  ICU 2.4

Definition at line 252 of file utf8.h.

#define U8_NEXT_UNSAFE | ( | s,
|  | i,
|  | c |  | ) |

Value:

    { \
        (c)=(uint8_t)(s)[(i)++]; \
        if((uint8_t)((c)-0xc0)<0x35) { \
            uint8_t __count=U8_COUNT_TRAIL_BYTES(c); \
            U8_MASK_LEAD_BYTE(c, __count); \
            switch(__count) { \
            /* each following branch falls through to the next one */ \
            case 3: \
                (c)=((c)<<6)|((s)[(i)++]&0x3f); \
            case 2: \
                (c)=((c)<<6)|((s)[(i)++]&0x3f); \
            case 1: \
                (c)=((c)<<6)|((s)[(i)++]&0x3f); \
            /* no other branches to optimize switch() */ \
                break; \
            } \
        } \
    }

Get a code point from a string at a code point boundary offset, and advance the offset to the next code point boundary.

(Post-incrementing forward iteration.) "Unsafe" macro, assumes well-formed UTF-8.

The offset may point to the lead byte of a multi-byte sequence, in which case the macro will read the whole sequence. The result is undefined if the offset points to a trail byte or an illegal UTF-8 sequence.

Parameters:

  | s | const uint8_t * string
  | i | string offset
  | c | output UChar32 variable

See also:
  U8_NEXT

Stable:
  ICU 2.4

Definition at line 215 of file utf8.h.

#define U8_PREV | ( | s,
|  | start,
|  | i,
|  | c |  | ) |

Value:

    { \
        (c)=(uint8_t)(s)[--(i)]; \
        if((c)>=0x80) { \
            if((c)<=0xbf) { \
                (c)=utf8_prevCharSafeBody((const uint8_t *)s, start, &(i), c, -1); \
            } else { \
                (c)=U_SENTINEL; \
            } \
        } \
    }

Move the string offset from one code point boundary to the previous one and get the code point between them.

(Pre-decrementing backward iteration.) "Safe" macro, checks for illegal sequences and for string boundaries.

The input offset may be the same as the string length. If the offset is behind a multi-byte sequence, then the macro will read the whole sequence. If the offset is behind a lead byte, then that itself will be returned as the code point. If the offset is behind an illegal UTF-8 sequence, then c is set to a negative value.

Parameters:

  | s | const uint8_t * string
  | start | starting string offset (usually 0)
  | i | string offset, must be start<i
  | c | output UChar32 variable, set to <0 in case of an error

See also:
  U8_PREV_UNSAFE

Stable:
  ICU 2.4

Definition at line 525 of file utf8.h.

#define U8_PREV_UNSAFE | ( | s,
|  | i,
|  | c |  | ) |

Value:

    { \
        (c)=(uint8_t)(s)[--(i)]; \
        if(U8_IS_TRAIL(c)) { \
            uint8_t __b, __count=1, __shift=6; \
    \
            /* c is a trail byte */ \
            (c)&=0x3f; \
            for(;;) { \
                __b=(uint8_t)(s)[--(i)]; \
                if(__b>=0xc0) { \
                    U8_MASK_LEAD_BYTE(__b, __count); \
                    (c)|=(UChar32)__b<<__shift; \
                    break; \
                } else { \
                    (c)|=(UChar32)(__b&0x3f)<<__shift; \
                    ++__count; \
                    __shift+=6; \
                } \
            } \
        } \
    }

Move the string offset from one code point boundary to the previous one and get the code point between them.

(Pre-decrementing backward iteration.) "Unsafe" macro, assumes well-formed UTF-8.

The input offset may be the same as the string length. If the offset is behind a multi-byte sequence, then the macro will read the whole sequence. If the offset is behind a lead byte, then that itself will be returned as the code point. The result is undefined if the offset is behind an illegal UTF-8 sequence.

Parameters:

  | s | const uint8_t * string
  | i | string offset
  | c | output UChar32 variable

See also:
  U8_PREV

Stable:
  ICU 2.4

Definition at line 483 of file utf8.h.

#define U8_SET_CP_LIMIT | ( | s,
|  | start,
|  | i,
|  | length |  | ) |

Value:

    { \
        if((start)<(i) && (i)<(length)) { \
            U8_BACK_1(s, start, i); \
            U8_FWD_1(s, i, length); \
        } \
    }

Adjust a random-access offset to a code point boundary after a code point.

If the offset is behind a partial multi-byte sequence, then the offset is incremented to behind the whole sequence. Otherwise, it is not modified. The input offset may be the same as the string length. "Safe" macro, checks for illegal sequences and for string boundaries.

Parameters:

  | s | const uint8_t * string
  | start | starting string offset (usually 0)
  | i | string offset, must be start<=i<=length
  | length | string length

See also:
  U8_SET_CP_LIMIT_UNSAFE

Stable:
  ICU 2.4

Definition at line 645 of file utf8.h.

#define U8_SET_CP_LIMIT_UNSAFE | ( | s,
|  | i |  | ) |

Value:

    { \
        U8_BACK_1_UNSAFE(s, i); \
        U8_FWD_1_UNSAFE(s, i); \
    }

Adjust a random-access offset to a code point boundary after a code point.

If the offset is behind a partial multi-byte sequence, then the offset is incremented to behind the whole sequence. Otherwise, it is not modified. The input offset may be the same as the string length. "Unsafe" macro, assumes well-formed UTF-8.

Parameters:

  | s | const uint8_t * string
  | i | string offset

See also:
  U8_SET_CP_LIMIT

Stable:
  ICU 2.4

Definition at line 625 of file utf8.h.

#define U8_SET_CP_START | ( | s,
|  | start,
|  | i |  | ) |

Value:

    { \
        if(U8_IS_TRAIL((s)[(i)])) { \
            (i)=utf8_back1SafeBody(s, start, (int32_t)(i)); \
        } \
    }

Adjust a random-access offset to a code point boundary at the start of a code point.

If the offset points to a UTF-8 trail byte, then the offset is moved backward to the corresponding lead byte. Otherwise, it is not modified. "Safe" macro, checks for illegal sequences and for string boundaries.

Parameters:

  | s | const uint8_t * string
  | start | starting string offset (usually 0)
  | i | string offset, must be start<=i

See also:
  U8_SET_CP_START_UNSAFE

Stable:
  ICU 2.4

Definition at line 456 of file utf8.h.

#define U8_SET_CP_START_UNSAFE | ( | s,
|  | i |  | ) |

Value:

    { \
        while(U8_IS_TRAIL((s)[i])) { --(i); } \
    }

Adjust a random-access offset to a code point boundary at the start of a code point.

If the offset points to a UTF-8 trail byte, then the offset is moved backward to the corresponding lead byte. Otherwise, it is not modified. "Unsafe" macro, assumes well-formed UTF-8.

Parameters:

  | s | const uint8_t * string
  | i | string offset

See also:
  U8_SET_CP_START

Stable:
  ICU 2.4

Definition at line 438 of file utf8.h.

## Function Documentation

int32_t utf8_appendCharSafeBody | ( | uint8_t * | s,
|  | int32_t | i,
|  | int32_t | length,
|  | UChar32 | c,
|  | UBool * | pIsError |
| ) |  |  |

Function for handling "append code point" with error-checking.

Internal:
  Do not use. This API is for internal use only.

int32_t utf8_back1SafeBody | ( | const uint8_t * | s,
|  | int32_t | start,
|  | int32_t | i |
| ) |  |  |

Function for handling "skip backward one code point" with error-checking.

Internal:
  Do not use. This API is for internal use only.

UChar32 utf8_nextCharSafeBody | ( | const uint8_t * | s,
|  | int32_t * | pi,
|  | int32_t | length,
|  | UChar32 | c,
|  | UBool | strict |
| ) |  |  |

Function for handling "next code point" with error-checking.

Internal:
  Do not use. This API is for internal use only.

UChar32 utf8_prevCharSafeBody | ( | const uint8_t * | s,
|  | int32_t | start,
|  | int32_t * | pi,
|  | UChar32 | c,
|  | UBool | strict |
| ) |  |  |

Function for handling "previous code point" with error-checking.

Internal:
  Do not use. This API is for internal use only.

## Variable Documentation

utf8_countTrailBytes

Internal array with numbers of trail bytes for any given byte used in lead byte position.

Internal:
  Do not use. This API is for internal use only.

Definition at line 57 of file utf8.h.