Next Previous Contents

## 3. Checking prerequisites.

You must ensure that any firewalls (either hardware, or a software firewall installed by your distribution) will not block access to the ports that will be used by the MythTV clients and servers on the "inside" LAN. The ports for MySQL (TCP port 3306) and mythbackend (TCP ports 6543 and 6544) must be open. It is strongly recommended that you do not expose the MythTV and MySQL ports to the Internet or your "Outside" LAN.

## 3.1 Hardware

Hardware selection is a complex topic, one this HOWTO will only discuss briefly and in general terms. The following subsections offer some general guidance but stop short of offering specific recommendations.

For a good MythTV experience, you must understand that MythTV exercises your hardware more than a typical desktop. Encoder cards generate DMA across the PCI bus. The CPU is busy encoding / decoding video. Hard drives are constantly reading and writing data. Building a MythTV system on older / "spare" hardware may be an exercise in frustration and can waste many hours of valuable time.

If you have specific questions about the suitability of specific hardware choices, you can consult the archives of the mythtv-users mailing list at http://www.gossamer-threads.com/lists/mythtv/ or post a question to the list.

### CPU Type and Speed

Selection of CPU type and speed is one of the trickiest elements of hardware selection, mainly because there are so many tradeoffs which can be made. For example, if you have plenty of CPU, you can use higher bitrates or capture sizes, etc.

### Software / CPU-based encoding.

MythTV has two modes of operation for capturing video. First, it can function as a software video encoder, which means that it can use a fairly generic "dumb" video capture card to get frames of video, encodes them using the CPU on your motherboard and writes them to disk. High-end video capture cards and devices like the TiVo and ReplayTV have dedicated encoder chips which use specialized hardware to convert the video stream to the MPEG-2 format without using the motherboard CPU. The main CPU has the responsibility of running the Operating System and reading and writing the encoded frames to the disk. These tasks have fairly low CPU requirements compared to encoding video, which is why a device like a Series 1 TiVo can run with only 16MB of RAM and a 54MHz CPU.

That being said, due to the digital conversion in the United States, there are fewer sources of NTSC analog video, and cheap silicon has made it easier to include MPEG-2 encoders into hardware capture cards. In addition, the sale of "analog-only" cards has been severely curtailed in the United States, and one vendor received a fine for failing to include notification that their device was analog-only. http://hraunfoss.fcc.gov/edocs_public/attachmatch/DA-08-493A1.txt

There are many variables that go into the question: "How fast a CPU do I need to run MythTV"? Obviously, the faster your CPU, the better your experience will be with MythTV. If you are using the software MPEG-4 encoder and performing the "Watch TV" function, where the CPU is both encoding and decoding video simultaneously to allow Pause, Fast Forward and Rewind functions for live TV requires more CPU then just encoding or decoding. MythTV also supports multiple encoder cards in a single PC, thereby increasing the CPU requirements if you plan on simultaneously encoding multiple programs. As a general guideline, plan on 1GHz per encoder if you are doing software-based encoding, less if you are using a hardware-based encoder.

Here are a few data points:

- A PIII/733MHz system can encode one video stream using the MPEG-4 codec using 480x480 capture resolution. This does not allow for live TV watching, but does allow for encoding video and then watching it later.
- A developer states that his AMD1800+ system can almost encode two MPEG-4 video streams and watch one program simultaneously.
- A PIII/800MHz system with 512MB RAM can encode one video stream using the RTjpeg codec with 480x480 capture resolution and play it back simultaneously, thereby allowing live TV watching.
- A dual Celeron/450MHz is able to view a 480x480 MPEG-4/3300kbps file created on a different system with 30% CPU usage.
- A P4 2.4GHz machine can encode two 3300Kbps 480x480 MPEG-4 files and simultaneously serve content to a remote frontend.

### Hardware based encoding.

The second mode of operation is where MythTV is paired with a hardware-based video encoder, in which case MythTV will primarily be I/O bound. There are several examples of such devices, like the Hauppauge WinTV-PVR-150/250/350/500 series, the Hauppauge HD-PVR (H.264 High-Def capture using Component inputs), or the Silicon Dust HDHomerun. In this mode, because the video encoding is being done by a dedicated video processor (the Hauppauge encoders), or the device is simply writing the data to disk (the HDHR and other digital devices, such as DVB cards) the host CPU requirements are quite low. See the Video Capture Device section for details.

Primary development in MythTV has transitioned to supporting MPEG-2 capture devices, H.264 and HDTV, so if given the option, go with the hardware encoder or choose a ATSC capture device. Because of the transition to digital broadcast in the United States, most television stations are now digital-only. There are still analog stations in the U.S., but a majority are low-powered. Canada still has analog broadcasts.

Analog encoding or hardware MPEG-2 encoding may still be required if you are trying to capture standard definition video sources, such as set-top-boxes.

### Memory

A MythTV host that is both a backend and a frontend and using software encoding with a single capture card should run adequately in 512MB of RAM. Additional RAM above 512MB will not necessarily increase performance, but may be useful if you are running multiple encoders.

### Hard Disk(s)

Encoded video takes up a lot of hard disk space. The exact amount depends on the encoding scheme, the size of the raw images and the frames per second, but typical values for MythTV range from 700 megabytes/hour for MPEG-4, 2 GB/hour for MPEG-2 and RTjpeg and 7 GB/hour for ATSC HDTV.

Writing video to disk is sensitive to timing issues; RTjpeg requires less CPU with the tradeoff being larger files and needing to write to the disk faster. MPEG-4 requires more CPU, but the files are smaller. At the default resolution, MPEG-2 creates the largest files of all with almost no CPU impact.

### Filesystems

MythTV creates large files, many in excess of 4GB. You must use a 64 or 128 bit filesystem. These will allow you to create large files. Filesystems known to have problems with large files are FAT (all versions), and ReiserFS (versions 3 and 4).

Because MythTV creates very large files, a filesystem that does well at deleting them is important. Numerous benchmarks show that XFS and JFS do very well at this task. You are strongly encouraged to consider one of these for your MythTV filesystem. JFS is the absolute best at deletion, so you may want to try it if XFS gives you problems. MythTV incorporates a "slow delete" feature, which progressively shrinks the file rather than attempting to delete it all at once, so if you're more comfortable with a filesystem such as ext3 (whose delete performance for large files isn't that good) you may use it rather than one of the known-good high-performance file systems. There are other ramifications to using XFS and JFS - neither offer the opportunity to shrink a filesystem; they may only be expanded.

NOTE: You must not use ReiserFS v3 for your recordings. You will get corrupted recordings if you do.

Because of the size of the MythTV files, it may be useful to plan for future expansion right from the beginning. If your case and power supply have the capacity for additional hard drives, read through the Advanced Partition Formatting sections for some pointers.

### Video Capture Device

In order to capture video, MythTV will need one or more video capture devices with Linux drivers. There are a number of classes of hardware available for capturing video.

### Frame Grabbers.

This class of card is the simplest and is usually the cheapest. There is no on-board encoding of the analog video; hardware known as a Digital-Analog Converter (DAC) takes the video and presents it to the computer in an essentially raw digital form.

For a list of video capture cards known to work with Linux, please see `/usr/src/linux/Documentation/video4linux/bttv` for a partial listing; even if your specific card is not listed, it may be that the vendor is actually using a standard reference design and placing their own name on it. See the video4linux mailing list ( https://listman.redhat.com/mailman/listinfo/video4linux-list) for more information and for specific hardware questions.

The most common inexpensive cards available use the Bt848, Bt878 or CX2388x series of video capture chips; examples are the "Hauppauge WinTV Go" card and the "AverTV Desktop PVR" card, both of which use the bttv kernel module.

    NOTE:  The ATI TV Wonder series and the ATI All-in-Wonder series of cards
    are not the same.  The All-in-Wonder cards will not work with MythTV.

NOTE: The ATI All-in-Wonder cards (which are not the same as the ATI TV Wonder, TV Wonder VE or TV Wonder Pro) will not work as a MythTV capture device because the GATOS http://gatos.sourceforge.net drivers that are available provide only a limited subset of the V4L API. The TV Wonder series of cards are supported by the Bt8x8 Video4Linux driver.

After you have installed a suitable capture device, you can check that the kernel sees it with `lspci`. Look for an entry labeled "Multimedia video controller". To get more detailed information about the card, use `lspci -v` or `lspci -vv`. Ensure that your system is loading the bttv modules by typing:

> `

>     # lsmod |grep bttv

> `

You want to see the `bttv` module listed.

### Hardware MPEG-2 encoders.

While inexpensive video-capture cards simply capture raw frames, leaving encoding to software, some higher-end cards incorporate hardware-based encoding. Using either a G200 MJPEG encoder card, or a MPEG-2 encoder card supported by the IvyTV project http://ivtvdriver.org such as the Hauppauge PVR-150/250/350/500, Avermedia M179, Hauppauge "Freestyle" or Yuan M600 cards will allow you to use dedicated hardware encoders rather than your CPU. Using the on-board MPEG-2 encoder greatly reduces the CPU requirements for encoding.

NOTE: Motherboards with the Via chipset are notoriously bad with DMA and have caused numerous issues with ivtv, including hard locks. See the ivtv website http://ivtvdriver.org for the latest information on what works and what doesn't.

Here are some data points for encoding:

- A Celeron 450 uses 2% CPU for encoding a 480x480 16Mbps MPEG-2 stream.

Here are some data points for decoding:

- An Athlon 1800XP can decode a 720x480 8Mbps MPEG-2 file using 10% CPU
- An Athlon 1GHz can decode a 720x480 16Mbps MPEG-2 file using 30-50% CPU, can decode a 480x480 16Mbps MPEG-2 using 30% CPU and approximately 30% for Live TV at 416x480.

### DVB capture cards.

DVB is a video standard primarily found in Europe (where it comes in DVB-C, DVB-T and DVB-S and -S2 varieties for Cable, Terrestrial and Satellite) and is also used as the programming interface for HDTV capture cards in Linux. To see if your DVB card is supported, see the list of cards in the "Supported Hardware" section of the DVB Wiki at http://www.linuxtv.org/wiki/index.php/Main_Page for more information.

In the United States, you may use a card such as the TwinHan to obtain unencrypted Free-To-Air satellite channels. See http://www.lyngsat.com/ for the types of content which are available.

### HDTV.

There are a number of HDTV cards with Linux drivers which are known to operate in the United States; a complete list of cards with DVB drivers can be found at http://www.linuxtv.org/ Some cards support capture of unencrypted digital cable TV (utilizing QAM64 or QAM256), others will only work with Over The Air signals captured with an antenna (with 8VSB).

None of the capture devices listed above perform any encoding; they merely allow your computer to save a copy of a HDTV stream which has already been converted to MPEG-2 at the broadcast facility.

### Hauppauge HD PVR

Hauppuage makes a device called the HD PVR, which accepts component HDTV signals and TOSLINK / SPDIF audio and performs a real-time encode into H.264. See http://www.hauppauge.com/site/products/data_hdpvr.html for additional information.

### Playback of HDTV using CPU

To playback HDTV content, plan on a powerful CPU if your video card does not provide support for offloading video decode. (See below for a description of VDPAU)

"How powerful?" depends on a number of factors, such as the capture resolution, whether the video is progressive or interlaced, and whether your display card has hardware-assist support for Linux.

The Simple Answer: Once you are in the 3.2 Ghz P4-class of CPU you should have no issues with viewing HDTV.

The Complicated Answer:

For 720p content (1280x720), a 2.4GHz P4 should be sufficient.

For 1920x1080i->1920x1080p with the better deinterlacing methods done in real time a 2.4GHz CPU is taxed, but should work if you use "Bob and Weave" deinterlacing, or if you have an NVIDIA card with video decode acceleration.

### Playback of HDTV using VDPAU

NVIDIA now incorporates MPEG-2 and H.264 decode acceleration in their binary driver; this is now officially supported in MythTV 0.22. Use of VDPAU offloads the decompression and deinterlacing of video to the video GPU rather than the CPU of the frontend, so the CPU requirements are drastically lowered. A fanless frontend using an Intel Atom CPU running a single-core at 1.6Ghz is sufficient to decode and deinterlace MPEG-2 and H.264 if it has VDPAU supported video.

### Firewire.

You may use the Firewire output of the Motorola DCT6200 or the SA3250. If your provider uses 5C encryption on a particular channel, you won't be able to get any content. Many users have resorted to using Firewire to change channels on their set-top-box and capture the High Def video using the Component output fed into a Hauppauge HD PVR.

### DBoxII or other devices running Neutrino

You may use the Ethernet port of an DBoxII or a similar device to capture MPEG-2. Your set top box has to be running the Neutrino GUI.

### USB Capture Devices.

The Plextor ConvertX PVR devices are supported through Linux drivers available from http://go7007.imploder.org/. MythTV uses the Plextor to capture hardware encoded MPEG-4, so the host CPU requirements are low.

Hauppauge WinTV-PVR-USB2 and variants are supported by the Linux Kernel as of 2.6.18. Additional information is available at http://www.isely.net/pvrusb2/).

### IP Recorder (RTSP, RTS, UDP)

MPEG-2, MPEG-4 and H.264 stream recording is supported using the IPTV recorder in MythTV. This recorder expects the channels to be supplied as a m3u playlist. If your DSL/Fiber provider supplies television service, but does not provide a m3u playlist for the channels, you can construct one for your own use. You do not need to download it from the same server as the streams themselves, and it can also be read from a file if this is more convenient.

NOTE: Some DSL providers only allow you to use one recorder at a time, so you may need to limit yourself to one recorder in MythTV and turn off any set top box the cable provider sold or rented to you with your service. This limitation is independent of the bandwidth you have purchased.

### Sound card

The system needs a sound card or an on-board equivalent on the motherboard to play back and in some cases, to record sound. Any sound card that can be operated by the ALSA (Advanced Linux Sound Architecture) kernel modules will work with MythTV. However, some cards and drivers will provide better quality or compatibility than others.

NOTE: Analog video capture cards are the only ones which require a sound card for capturing audio. DVB, HDTV, and other hardware encoder cards all provide a combined audio / video stream. If you're not using a V4L analog device, you may skip this section.

The usual practice for capturing the audio associated with the video is to run a cable from an audio output on the video capture card to the Line input on a sound card. However, some video capture cards provide on-board audio capabilities that work with the kernel `btaudio` module instead, thereby eliminating the need for a cable. This is useful if you will be using multiple capture cards in a single chassis, since each capture card will not need its own sound card. Note that a separate sound card is still required for playback when using `btaudio`, and that often the audio recorded in this way will be mono only. See the btaudio section for more information.

NOTE: Plugging a Line-level device into the Mic input is not recommended. Line-level devices have higher voltages and can damage the sound card. In addition, even if it doesn't break your card, you will be getting Mono sound. See the Linux MP3 HOWTO at http://www.tldp.org/HOWTO/MP3-HOWTO.html for additional information.

### Video Display Card

MythTV will work with just about any video card. However, it is highly recommended that you use a card which supports XVideo (XV) extensions. If your card does not support XV, color conversion and scaling will be performed by your CPU rather than the video card. This is very CPU and memory intensive and will often result in dropped frames and a corresponding degradation of quality. Check the X documentation for details if you are uncertain about your preferred card. You may also run `xvinfo`; look for your video card to be listed as one of the adapters.

If you want to use MythTV with a standard television, you will need a physical connection from your video card to your TV set, which can either be a TV-out port on the card itself or an external adapter that converts the VGA signal to an appropriate video signal. "Appropriate" depends on a number of factors, such as video standard (NTSC vs. PAL), the type of input connection (Composite vs. SVideo), etc.

Note that with some video cards and X drivers, XVideo extensions are only supported on the VGA output, and not on the TV output.

### Cards with TV-out

This section deals with a number of cards that are known to have TV-out ports. The list is unlikely to be complete, so if you know of others, please post a message to the mythtv-users mailing list so the information can be included in future versions of the HOWTO. The list is organized by manufacturer.

Reports here are based on what users of the cards have posted on the mythtv-users mailing list, so if you need configuration details, please search the archives at http://www.gossamer-threads.com/lists/mythtv/ using the card name in your search string.

### ATI

ATI makes many cards with TV-out capability, but only offers Linux drivers for Radeon 8500 and above cards. See the Drivers and Software section of http://www.ati.com for the driver and additional information.

The enhanced ati.2 X driver created by the GATOS http://gatos.sourceforge.net project offers some support for TV-out on other ATI cards, but only in its "experimental" version, available through CVS. There have been reports from people who say they have made this driver work with one or another ATI card. For example, Bruce Markey mailto:bjm@lvcm.com writes (on the mythtv-users mailing list): "I got this to work. You can quote me on that. I've used TV-out on several models of ATI cards both All-In-Wonder and regular cards with TV-out." See the "Adventurous Setup" section of http://gatos.sourceforge.net/watching_tv.php for details. Also see http://www.retinalburn.net/linux/tvout.html for more information.

### NVIDIA

Some NVIDIA cards with TV-out can be run using the standard nv driver in X, combined with the userspace application nvtv to control the TV-out port. See http://sourceforge.net/projects/nv-tv-out/ for details. Recent versions of the NVIDIA driver have better support for overscan and other features useful with TV-Out, so the nvtv application may not be required.

Some NVIDIA cards can be run with a proprietary NVIDIA X driver made available by NVIDIA. See http://www.nvidia.com/object/unix.html for more information.

NOTE: It's strongly recommended that you use the proprietary NVIDIA drivers; they have excellent support for XvMC and ship with a good configuration utility. XvMC provides MPEG-2 hardware acceleration, which is important if you want to display HDTV. VDPAU is another new feature and it provides an API for offloading MPEG-2 and H.264 to the GPU.

### Hauppauge PVR-350

As of MythTV 0.22, the TV-out and MPEG-2 decoder functions of the PVR-350 are no longer supported. This functionality is currently unmaintained, and will be removed in MythTV 0.23.

### External Adapters

External adapters convert standard VGA output to a form suitable for display on a television. The output format varies by region, since different countries have different TV standards. People on the mythtv-users list have mentioned these adapters:

- AITech Web Cable Plus, powered by external transformer or takes power from PS/2 keyboard connector, support resolutions up to 1024x768, outputs composite and SVideo, provides position adjustment.
- Averkey lite, powered by a USB port, has Composite, SVideo, YPbPr outputs; pan, brightness, overscan/underscan controls; supports up to 1024x768 outputs; and supports PAL and NTSC.
- ADS TV Elite XGA
- AverKey iMicro (comments are generally favorable)
- AITech Web Cable (comments are generally unfavorable, different than the "Plus" version above)
- TVIEW Gold (mentioned once, favorably)

## 3.2 Software

There are a few ways of installing programs on Linux systems; you can either use a pre-compiled package, or install from a tarball after satisfying any prerequisites.

NOTE: you must have the MySQL database software installed on a system to store the master database. This does not necessarily mean that MySQL must run on one of the MythTV boxes. The minimum MySQL version is 5.0.15.

### Pre-compiled packages

A number of people have created pre-compiled packages for MythTV that may make your installation easier.

BIG FAT WARNING: This HOWTO assumes that you have not installed MythTV from a package. All example command lines and file locations are based on the MythTV tarball defaults. Some packagers have modified the filenames, binaries and file locations to match what is commonly found in that distribution. Any issues with MythTV installed via a pre-compiled package MUST be raised with the packager.

If you use any of the pre-compiled packages you may not need to perform any additional configuration steps in this HOWTO. The next logical step is configuring MySQL, which you may or may not have to perform. See your package documentation.

### Red Hat Linux / Fedora Core / MythDora

The definitive documentation on installing MythTV on Red Hat Linux / Fedora Core can be found in Jarod Wilson's ( mailto:jcw@wilsonet.com) HOWTO at http://wilsonet.com/mythtv/ Just like 3rd-party packages, any 3rd-party documentation problems should be brought up with the 3rd-parties (maintainer, lists, bugzillas etc.).

### Debian

Debian packages for MythTV and most of its add-on modules are maintained by Christian Marillat mailto:marillat@free.fr and are available at http://www.debian-multimedia.org/. Installation instructions can be found on those pages as well. All of the prerequisites for MythTV are available as Debian packages, most of them from the official Debian archive.

After adding the appropriate commands to your `/etc/apt/sources.list` file you can run apt-get update and then execute apt-get build-dep mythtv which should install all the pre-requisites required to compile MythTV.

### Manual installation

You may use the graphical tools that come with your distribution, or you can use command-line utilities. Either system will get the job done, and it all depends on your comfort level with Linux.

In order to compile MythTV, we need to make sure that the software it needs is installed. This list includes mysql, gcc, freetype2-devel, xorg-xserver-devel, qt-devel and lame. If you're going to use a remote control with MythTV, you're going to need the cdialog package in order to compile lircd if your distribution doesn't have a pre-packaged lirc. If you are using XMLTV as a grabber, you will need perl.

    NOTE:  Qt v4.4 or higher is required.

    NOTE:  If you are going to be using packages to install various
    components, you should be aware that not all packages include the necessary
    headers for compiling.  If you're having trouble compiling, ensure
    that you've installed the -devel version of a prerequisite.

### Command-line installation

This section details the various methods for installing prerequisites from the command line.

### Fedora / Mythdora

Assuming that you've configured ATrpms, you can execute:

> `

>     # yum-builddep mythtv

> `

Alternatively, you may use the build script located in `packaging/rpm`, or install the "requires" found in the mythtv.spec file located in the same directory.

### Mythbuntu

You can run

> `

>     $ sudo apt-get build-dep mythtv

> `

### Debian.

Build-dependencies for MythTV can be satisfied by adding the following to your `/etc/apt/sources.list`

> `

>     # Christian Marillat's packages (mplayer, lame)
>     deb http://www.debian-multimedia.org sid main
>     deb-src http://www.debian-multimedia.org sid main

> `

and executing:

> `

>     # apt-get build-dep mythtv
>     # apt-get source mythtv --compile

> `

Next Previous Contents