### Navigation

- index
- modules |
- modules |
- next |
- previous |
- SciPy v0.12 Reference Guide (DRAFT) »
- Signal processing (`scipy.signal`) »

# scipy.signal.bode

`scipy.signal.``bode`(system, w=None, n=100)

  Calculate bode magnitude and phase data of a continuous-time system.

  New in version 0.11.0.

  Parameters : | system : an instance of the LTI class or a tuple describing the system. The following gives the number of elements in the tuple and the interpretation: 2 (num, den) 3 (zeros, poles, gain) 4 (A, B, C, D) w : array_like, optional Array of frequencies (in rad/s). Magnitude and phase data is calculated for every value in this array. If not given a reasonable set will be calculated. n : int, optional Number of frequency points to compute if w is not given. The n frequencies are logarithmically spaced in the range from two orders of magnitude before the minimum (slowest) pole to two orders of magnitude after the maximum (fastest) pole.
  Returns : | w : 1D ndarray Frequency array [rad/s] mag : 1D ndarray Magnitude array [dB] phase : 1D ndarray Phase array [deg]

  Examples

      >>> from scipy import signal
      >>> import matplotlib.pyplot as plt

      >>> s1 = signal.lti([1], [1, 1])
      >>> w, mag, phase = signal.bode(s1)

      >>> plt.figure()
      >>> plt.semilogx(w, mag)    # bode magnitude plot
      >>> plt.figure()
      >>> plt.semilogx(w, phase)  # bode phase plot
      >>> plt.show()

  (Source code)

### Navigation

- index
- modules |
- modules |
- next |
- previous |
- SciPy v0.12 Reference Guide (DRAFT) »
- Signal processing (`scipy.signal`) »