### Navigation

- index
- modules |
- modules |
- next |
- previous |
- SciPy v0.12 Reference Guide (DRAFT) »
- Signal processing (`scipy.signal`) »

# scipy.signal.blackman

`scipy.signal.``blackman`(M, sym=True)

  Return a Blackman window.

  The Blackman window is a taper formed by using the the first three terms of a summation of cosines. It was designed to have close to the minimal leakage possible. It is close to optimal, only slightly worse than a Kaiser window.

  Parameters : | M : int Number of points in the output window. If zero or less, an empty array is returned. sym : bool, optional When True, generates a symmetric window, for use in filter design. When False, generates a periodic window, for use in spectral analysis.
  Returns : | w : ndarray The window, with the maximum value normalized to 1 (though the value 1 does not appear if the number of samples is even and sym is True).

  Notes

  The Blackman window is defined as

  Most references to the Blackman window come from the signal processing literature, where it is used as one of many windowing functions for smoothing values. It is also known as an apodization (which means “removing the foot”, i.e. smoothing discontinuities at the beginning and end of the sampled signal) or tapering function. It is known as a “near optimal” tapering function, almost as good (by some measures) as the Kaiser window.

  References

  [R95] | Blackman, R.B. and Tukey, J.W., (1958) The measurement of power spectra, Dover Publications, New York.

  [R96] | Oppenheim, A.V., and R.W. Schafer. Discrete-Time Signal Processing. Upper Saddle River, NJ: Prentice-Hall, 1999, pp. 468-471.

  Examples

  Plot the window and its frequency response:

      >>> from scipy import signal
      >>> from scipy.fftpack import fft, fftshift
      >>> import matplotlib.pyplot as plt

      >>> window = signal.blackman(51)
      >>> plt.plot(window)
      >>> plt.title("Blackman window")
      >>> plt.ylabel("Amplitude")
      >>> plt.xlabel("Sample")

      >>> plt.figure()
      >>> A = fft(window, 2048) / (len(window)/2.0)
      >>> freq = np.linspace(-0.5, 0.5, len(A))
      >>> response = 20 * np.log10(np.abs(fftshift(A / abs(A).max())))
      >>> plt.plot(freq, response)
      >>> plt.axis([-0.5, 0.5, -120, 0])
      >>> plt.title("Frequency response of the Blackman window")
      >>> plt.ylabel("Normalized magnitude [dB]")
      >>> plt.xlabel("Normalized frequency [cycles per sample]")

  (Source code)

### Navigation

- index
- modules |
- modules |
- next |
- previous |
- SciPy v0.12 Reference Guide (DRAFT) »
- Signal processing (`scipy.signal`) »