### Navigation

- index
- modules |
- modules |
- next |
- previous |
- SciPy v0.12 Reference Guide (DRAFT) »
- Signal processing (`scipy.signal`) »

# scipy.signal.symiirorder2

`scipy.signal.``symiirorder2`(input, r, omega {, precision}) → output

  Implement a smoothing IIR filter with mirror-symmetric boundary conditions using a cascade of second-order sections. The second section uses a reversed sequence. This implements the following transfer function:

                               cs^2
      H(z) = ---------------------------------------
             (1 - a2/z - a3/z^2) (1 - a2 z - a3 z^2 )

  where:

      a2 = (2 r cos omega)
      a3 = - r^2
      cs = 1 - 2 r cos omega + r^2

  Parameters : | input : ndarray The input signal. r, omega : scalar Parameters in the transfer function. precision : : Specifies the precision for calculating initial conditions of the recursive filter based on mirror-symmetric input.
  Returns : | output : ndarray The filtered signal.

### Navigation

- index
- modules |
- modules |
- next |
- previous |
- SciPy v0.12 Reference Guide (DRAFT) »
- Signal processing (`scipy.signal`) »