# scipy.signal.iirfilter

scipy.signal.iirfilter(N, Wn, rp=None, rs=None, btype='band', analog=False, ftype='butter', output='ba', fs=None)

  IIR digital and analog filter design given order and critical points.

  Design an Nth-order digital or analog filter and return the filter coefficients.

  Parameters
    N int

      The order of the filter.

    Wn array_like

      A scalar or length-2 sequence giving the critical frequencies.

      For digital filters, Wn are in the same units as fs. By default, fs is 2 half-cycles/sample, so these are normalized from 0 to 1, where 1 is the Nyquist frequency. (Wn is thus in half-cycles / sample.)

      For analog filters, Wn is an angular frequency (e.g., rad/s).

    rp float, optional

      For Chebyshev and elliptic filters, provides the maximum ripple in the passband. (dB)

    rs float, optional

      For Chebyshev and elliptic filters, provides the minimum attenuation in the stop band. (dB)

    btype{‘bandpass’, ‘lowpass’, ‘highpass’, ‘bandstop’}, optional

      The type of filter. Default is ‘bandpass’.

    analog bool, optional

      When True, return an analog filter, otherwise a digital filter is returned.

    ftype str, optional

      The type of IIR filter to design:

      > - Butterworth : ‘butter’

      > - Chebyshev I : ‘cheby1’

      > - Chebyshev II : ‘cheby2’

      > - Cauer/elliptic: ‘ellip’

      > - Bessel/Thomson: ‘bessel’

    output{‘ba’, ‘zpk’, ‘sos’}, optional

      Filter form of the output:

      > - second-order sections (recommended): ‘sos’

      > - numerator/denominator (default) : ‘ba’

      > - pole-zero : ‘zpk’

      In general the second-order sections (‘sos’) form is recommended because inferring the coefficients for the numerator/denominator form (‘ba’) suffers from numerical instabilities. For reasons of backward compatibility the default form is the numerator/denominator form (‘ba’), where the ‘b’ and the ‘a’ in ‘ba’ refer to the commonly used names of the coefficients used.

      Note: Using the second-order sections form (‘sos’) is sometimes associated with additional computational costs: for data-intense use cases it is therefore recommended to also investigate the numerator/denominator form (‘ba’).

    fs float, optional

      The sampling frequency of the digital system.

      New in version 1.2.0.

  Returns
    b, a ndarray, ndarray

      Numerator (b) and denominator (a) polynomials of the IIR filter. Only returned if `output='ba'`.

    z, p, k ndarray, ndarray, float

      Zeros, poles, and system gain of the IIR filter transfer function. Only returned if `output='zpk'`.

    sos ndarray

      Second-order sections representation of the IIR filter. Only returned if `output=='sos'`.

  See also

  `butter`

    Filter design using order and critical points

  `cheby1`, `cheby2`, `ellip`, `bessel`
  `buttord`

    Find order and critical points from passband and stopband spec

  `cheb1ord`, `cheb2ord`, `ellipord`
  `iirdesign`

    General filter design using passband and stopband spec

  Notes

  The `'sos'` output parameter was added in 0.16.0.

  Examples

  Generate a 17th-order Chebyshev II analog bandpass filter from 50 Hz to 200 Hz and plot the frequency response:

      >>> from scipy import signal
      >>> import matplotlib.pyplot as plt

      >>> b, a = signal.iirfilter(17, [2*np.pi*50, 2*np.pi*200], rs=60,
      ...                         btype='band', analog=True, ftype='cheby2')
      >>> w, h = signal.freqs(b, a, 1000)
      >>> fig = plt.figure()
      >>> ax = fig.add_subplot(1, 1, 1)
      >>> ax.semilogx(w / (2*np.pi), 20 * np.log10(np.maximum(abs(h), 1e-5)))
      >>> ax.set_title('Chebyshev Type II bandpass frequency response')
      >>> ax.set_xlabel('Frequency [Hz]')
      >>> ax.set_ylabel('Amplitude [dB]')
      >>> ax.axis((10, 1000, -100, 10))
      >>> ax.grid(which='both', axis='both')
      >>> plt.show()

  Create a digital filter with the same properties, in a system with sampling rate of 2000 Hz, and plot the frequency response. (Second-order sections implementation is required to ensure stability of a filter of this order):

      >>> sos = signal.iirfilter(17, [50, 200], rs=60, btype='band',
      ...                        analog=False, ftype='cheby2', fs=2000,
      ...                        output='sos')
      >>> w, h = signal.sosfreqz(sos, 2000, fs=2000)
      >>> fig = plt.figure()
      >>> ax = fig.add_subplot(1, 1, 1)
      >>> ax.semilogx(w, 20 * np.log10(np.maximum(abs(h), 1e-5)))
      >>> ax.set_title('Chebyshev Type II bandpass frequency response')
      >>> ax.set_xlabel('Frequency [Hz]')
      >>> ax.set_ylabel('Amplitude [dB]')
      >>> ax.axis((10, 1000, -100, 10))
      >>> ax.grid(which='both', axis='both')
      >>> plt.show()

scipy.signal.iirdesign scipy.signal.kaiser_atten