# scipy.signal.lp2bp_zpk

scipy.signal.lp2bp_zpk(z, p, k, wo=1.0, bw=1.0)

  Transform a lowpass filter prototype to a bandpass filter.

  Return an analog band-pass filter with center frequency wo and bandwidth bw from an analog low-pass filter prototype with unity cutoff frequency, using zeros, poles, and gain (‘zpk’) representation.

  Parameters
    z array_like

      Zeros of the analog filter transfer function.

    p array_like

      Poles of the analog filter transfer function.

    k float

      System gain of the analog filter transfer function.

    wo float

      Desired passband center, as angular frequency (e.g., rad/s). Defaults to no change.

    bw float

      Desired passband width, as angular frequency (e.g., rad/s). Defaults to 1.

  Returns
    z ndarray

      Zeros of the transformed band-pass filter transfer function.

    p ndarray

      Poles of the transformed band-pass filter transfer function.

    k float

      System gain of the transformed band-pass filter.

  See also

  `lp2lp_zpk`, `lp2hp_zpk`, `lp2bs_zpk`, `bilinear`
  `lp2bp`

  Notes

  This is derived from the s-plane substitution

  \[s \rightarrow \frac{s^2 + {\omega_0}^2}{s \cdot \mathrm{BW}}\]

  This is the “wideband” transformation, producing a passband with geometric (log frequency) symmetry about wo.

  New in version 1.1.0.

scipy.signal.lp2bp scipy.signal.lp2bs