# scipy.signal.resample

scipy.signal.resample(x, num, t=None, axis=0, window=None, domain='time')

  Resample x to num samples using Fourier method along the given axis.

  The resampled signal starts at the same value as x but is sampled with a spacing of `len(x) / num * (spacing of x)`. Because a Fourier method is used, the signal is assumed to be periodic.

  Parameters
    x array_like

      The data to be resampled.

    num int

      The number of samples in the resampled signal.

    t array_like, optional

      If t is given, it is assumed to be the equally spaced sample positions associated with the signal data in x.

    axis int, optional

      The axis of x that is resampled. Default is 0.

    window array_like, callable, string, float, or tuple, optional

      Specifies the window applied to the signal in the Fourier domain. See below for details.

    domain string, optional

      A string indicating the domain of the input x: `time` Consider the input x as time-domain (Default), `freq` Consider the input x as frequency-domain.

  Returns
    resampled_x or (resampled_x, resampled_t)

      Either the resampled array, or, if t was given, a tuple containing the resampled array and the corresponding resampled positions.

  See also

  `decimate`

    Downsample the signal after applying an FIR or IIR filter.

  `resample_poly`

    Resample using polyphase filtering and an FIR filter.

  Notes

  The argument window controls a Fourier-domain window that tapers the Fourier spectrum before zero-padding to alleviate ringing in the resampled values for sampled signals you didn’t intend to be interpreted as band-limited.

  If window is a function, then it is called with a vector of inputs indicating the frequency bins (i.e. fftfreq(x.shape[axis]) ).

  If window is an array of the same length as x.shape[axis] it is assumed to be the window to be applied directly in the Fourier domain (with dc and low-frequency first).

  For any other type of window, the function `scipy.signal.get_window` is called to generate the window.

  The first sample of the returned vector is the same as the first sample of the input vector. The spacing between samples is changed from `dx` to `dx * len(x) / num`.

  If t is not None, then it is used solely to calculate the resampled positions resampled_t

  As noted, `resample` uses FFT transformations, which can be very slow if the number of input or output samples is large and prime; see `scipy.fft.fft`.

  Examples

  Note that the end of the resampled data rises to meet the first sample of the next cycle:

      >>> from scipy import signal

      >>> x = np.linspace(0, 10, 20, endpoint=False)
      >>> y = np.cos(-x**2/6.0)
      >>> f = signal.resample(y, 100)
      >>> xnew = np.linspace(0, 10, 100, endpoint=False)

      >>> import matplotlib.pyplot as plt
      >>> plt.plot(x, y, 'go-', xnew, f, '.-', 10, y[0], 'ro')
      >>> plt.legend(['data', 'resampled'], loc='best')
      >>> plt.show()

scipy.signal.detrend scipy.signal.resample_poly