# scipy.signal.square

scipy.signal.square(t, duty=0.5)

  Return a periodic square-wave waveform.

  The square wave has a period `2*pi`, has value +1 from 0 to `2*pi*duty` and -1 from `2*pi*duty` to `2*pi`. duty must be in the interval [0,1].

  Note that this is not band-limited. It produces an infinite number of harmonics, which are aliased back and forth across the frequency spectrum.

  Parameters
    t array_like

      The input time array.

    duty array_like, optional

      Duty cycle. Default is 0.5 (50% duty cycle). If an array, causes wave shape to change over time, and must be the same length as t.

  Returns
    y ndarray

      Output array containing the square waveform.

  Examples

  A 5 Hz waveform sampled at 500 Hz for 1 second:

      >>> from scipy import signal
      >>> import matplotlib.pyplot as plt
      >>> t = np.linspace(0, 1, 500, endpoint=False)
      >>> plt.plot(t, signal.square(2 * np.pi * 5 * t))
      >>> plt.ylim(-2, 2)

  A pulse-width modulated sine wave:

      >>> plt.figure()
      >>> sig = np.sin(2 * np.pi * t)
      >>> pwm = signal.square(2 * np.pi * 30 * t, duty=(sig + 1)/2)
      >>> plt.subplot(2, 1, 1)
      >>> plt.plot(t, sig)
      >>> plt.subplot(2, 1, 2)
      >>> plt.plot(t, pwm)
      >>> plt.ylim(-1.5, 1.5)

scipy.signal.sawtooth scipy.signal.sweep_poly