Overview | Package | Class | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES

# Constant Field Values

Contents

- com.sun.*

com.sun.*

com.sun.javacard.apduio.Apdu
`public static final int` | `APDU_TYPE_MASK` | `240`
`public static final int` | `CASE_1` | `1`
`public static final int` | `CASE_2E` | `5`
`public static final int` | `CASE_2S` | `2`
`public static final int` | `CASE_3E` | `6`
`public static final int` | `CASE_3S` | `3`
`public static final int` | `CASE_4E` | `7`
`public static final int` | `CASE_4S` | `4`
`public static final int` | `CLA` | `0`
`public static final int` | `COMMAND_ARRAY_SIZE` | `6`
`public static final int` | `INS` | `1`
`public static final int` | `LOGICAL_CHN_MASK` | `3`
`public static final int` | `P1` | `2`
`public static final int` | `P2` | `3`
`public static final int` | `P3` | `4`

com.sun.javacard.apduio.CadDevice
`public static final byte` | `PROTOCOL_PCSC` | `-85`
`public static final byte` | `PROTOCOL_T0` | `0`
`public static final byte` | `PROTOCOL_T1` | `1`
`public static final byte` | `PROTOCOL_TCL` | `91`

com.sun.javacard.apduio.CadT1
`protected static final int` | `MAX_IFS_SIZE` | `32`

com.sun.javacard.apduio.CadT1Dual
`protected static final int` | `MAX_IFS_SIZE` | `32`

com.sun.javacard.apduio.T1Block
`public static final byte` | `NULL_ADDRESS` | `0`
`public static final byte` | `S_ABORT_REQ` | `-62`
`public static final byte` | `S_ABORT_RES` | `-30`
`public static final byte` | `S_IFS_REQ` | `-63`
`public static final byte` | `S_IFS_RES` | `-31`
`public static final byte` | `S_RESYNC_REQ` | `-64`
`public static final byte` | `S_RESYNC_RES` | `-32`
`public static final byte` | `S_WTX_REQ` | `-61`
`public static final byte` | `S_WTX_RES` | `-29`

com.sun.javacard.apduio.T1Exception
`public static final int` | `T1_BAD_CHECKSUM` | `-123`
`public static final int` | `T1_BLOCK_IO_ERROR` | `-126`
`public static final int` | `T1_FUNCTION_NOT_SUPPORTED` | `-125`
`public static final int` | `T1_PROTOCOL_VIOLATION` | `-124`
`public static final int` | `T1_UNINITIALIZED` | `-127`
`public static final int` | `T1_WRONG_LENGTH` | `-128`

com.sun.javacard.apduio.TLP224Message
`public static final int` | `ACK` | `96`
`public static final int` | `EOT` | `3`
`public static final int` | `ISO_INPUT` | `218`
`public static final int` | `ISO_OUTPUT` | `219`
`public static final int` | `MAX_MESSAGE_LEN` | `258`
`public static final int` | `NACK` | `224`
`public static final int` | `POWER_DOWN` | `77`
`public static final int` | `POWER_UP` | `110`
`public static final int` | `STATUS_CARD_ABORTED_CHAINING` | `164`
`public static final int` | `STATUS_CARD_ERROR` | `231`
`public static final int` | `STATUS_CARD_MALFUNCTION` | `162`
`public static final int` | `STATUS_CARD_MISSING` | `251`
`public static final int` | `STATUS_CARD_PROTOCOL_ERROR` | `161`
`public static final int` | `STATUS_CARD_REMOVED` | `247`
`public static final int` | `STATUS_CARD_TURNED_OFF` | `21`
`public static final int` | `STATUS_COMMAND_UNKNOWN` | `4`
`public static final int` | `STATUS_INCORRECT_NUMBER_OF_ARGS` | `3`
`public static final int` | `STATUS_INTERRUPTED_EXCHANGE` | `229`
`public static final int` | `STATUS_INVALID_PROCEDURE_BYTE` | `228`
`public static final int` | `STATUS_ISO_CMD_ERROR` | `17`
`public static final int` | `STATUS_ISO_LC_ERROR` | `26`
`public static final int` | `STATUS_MESSAGE_TOO_LONG` | `18`
`public static final int` | `STATUS_PROTOCOL_ERROR` | `9`
`public static final int` | `STATUS_READER_ABORTED_CHAINING` | `165`
`public static final int` | `STATUS_SUCCESS` | `0`
`public static final int` | `STATUS_UNKNOWN_PROTOCOL` | `23`

Overview | Package | Class | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES

Copyright (c) 2009 Sun Microsystems, Inc. All rights reserved.