### Navigation

- index
- modules |
- modules |
- next |
- previous |
- SciPy v0.12 Reference Guide (DRAFT) »
- Signal processing (`scipy.signal`) »

# scipy.signal.qspline1d

`scipy.signal.``qspline1d`(signal, lamb=0.0)

  Compute quadratic spline coefficients for rank-1 array.

  Find the quadratic spline coefficients for a 1-D signal assuming mirror-symmetric boundary conditions. To obtain the signal back from the spline representation mirror-symmetric-convolve these coefficients with a length 3 FIR window [1.0, 6.0, 1.0]/ 8.0 .

  Parameters : | signal : ndarray A rank-1 array representing samples of a signal. lamb : float, optional Smoothing coefficient (must be zero for now).
  Returns : | c : ndarray Cubic spline coefficients.

### Navigation

- index
- modules |
- modules |
- next |
- previous |
- SciPy v0.12 Reference Guide (DRAFT) »
- Signal processing (`scipy.signal`) »