### Navigation

- index
- modules |
- next |
- previous |
- SciPy v0.7 Reference Guide (DRAFT) »
- Signal processing (`scipy.signal`) »

# scipy.signal.get_window

`scipy.signal.``get_window`(window, Nx, fftbins=1)

  Return a window of length Nx and type window.

  If fftbins is 1, create a “periodic” window ready to use with ifftshift and be multiplied by the result of an fft (SEE ALSO fftfreq).

  Window types: boxcar, triang, blackman, hamming, hanning, bartlett,
    parzen, bohman, blackmanharris, nuttall, barthann, kaiser (needs beta), gaussian (needs std), general_gaussian (needs power, width), slepian (needs width)

  If the window requires no parameters, then it can be a string. If the window requires parameters, the window argument should be a tuple

  > with the first argument the string name of the window, and the next arguments the needed parameters.

  If window is a floating point number, it is interpreted as the beta
    parameter of the kaiser window.

### Navigation

- index
- modules |
- next |
- previous |
- SciPy v0.7 Reference Guide (DRAFT) »
- Signal processing (`scipy.signal`) »