### Navigation

- index
- modules |
- modules |
- next |
- previous |
- SciPy v0.9 Reference Guide (DRAFT) »
- Signal processing (`scipy.signal`) »

# scipy.signal.kaiserord

`scipy.signal.``kaiserord`(ripple, width)

  Design a Kaiser window to limit ripple and width of transition region.

  Parameters : | ripple : float Positive number specifying maximum ripple in passband (dB) and minimum ripple in stopband. width : float Width of transition region (normalized so that 1 corresponds to pi radians / sample).
  Returns : | numtaps : int The length of the kaiser window. beta : : The beta parameter for the kaiser window.

  See also

  `kaiser_beta`, `kaiser_atten`

  Notes

  There are several ways to obtain the Kaiser window:

  > signal.kaiser(numtaps, beta, sym=0) signal.get_window(beta, numtaps) signal.get_window((‘kaiser’, beta), numtaps)

  The empirical equations discovered by Kaiser are used.

  References

  Oppenheim, Schafer, “Discrete-Time Signal Processing”, p.475-476.

### Navigation

- index
- modules |
- modules |
- next |
- previous |
- SciPy v0.9 Reference Guide (DRAFT) »
- Signal processing (`scipy.signal`) »