Small. Fast. Reliable.
Choose any three.

About Sitemap Documentation Download License News Developers Support

## SQLite C Interface

## Device Characteristics

>     #define SQLITE_IOCAP_ATOMIC          0x00000001
>     #define SQLITE_IOCAP_ATOMIC512       0x00000002
>     #define SQLITE_IOCAP_ATOMIC1K        0x00000004
>     #define SQLITE_IOCAP_ATOMIC2K        0x00000008
>     #define SQLITE_IOCAP_ATOMIC4K        0x00000010
>     #define SQLITE_IOCAP_ATOMIC8K        0x00000020
>     #define SQLITE_IOCAP_ATOMIC16K       0x00000040
>     #define SQLITE_IOCAP_ATOMIC32K       0x00000080
>     #define SQLITE_IOCAP_ATOMIC64K       0x00000100
>     #define SQLITE_IOCAP_SAFE_APPEND     0x00000200
>     #define SQLITE_IOCAP_SEQUENTIAL      0x00000400

The xDeviceCapabilities method of the sqlite3_io_methods object returns an integer which is a vector of the these bit values expressing I/O characteristics of the mass storage device that holds the file that the sqlite3_io_methods refers to.

The SQLITE_IOCAP_ATOMIC property means that all writes of any size are atomic. The SQLITE_IOCAP_ATOMICnnn values mean that writes of blocks that are nnn bytes in size and are aligned to an address which is an integer multiple of nnn are atomic. The SQLITE_IOCAP_SAFE_APPEND value means that when data is appended to a file, the data is appended first then the size of the file is extended, never the other way around. The SQLITE_IOCAP_SEQUENTIAL property means that information is written to disk in the same order as calls to xWrite().

See also lists of Objects, Constants, and Functions.

This page last modified 2009/02/18 18:03:35 UTC